1. Load sketch to **Arduino Uno**
2. Open “RGBLamp” binary file in “Binary” folder
3. Connect RGB Diode by next instruction:
   1. R-3
   2. G-5
   3. B-6
4. Connect Arduino to PC (install CH341 driver to use)
5. Get number of COM port (COMx) to connect program to Arduino

DONE! ENJOY!